#MicroXplorer Configuration settings - do not modify
CAD.formats=
CAD.pinconfig=
CAD.provider=
CORTEX_M7.CPU_ICache=Disabled
CORTEX_M7.IPParameters=PREFETCH_ENABLE,CPU_ICache
CORTEX_M7.PREFETCH_ENABLE=0
FREERTOS.IPParameters=Tasks01,configTOTAL_HEAP_SIZE,configGENERATE_RUN_TIME_STATS,configUSE_TRACE_FACILITY,configUSE_NEWLIB_REENTRANT
FREERTOS.Tasks01=defaultTask,0,256,StartDefaultTask,Default,NULL,Dynamic,NULL,NULL
FREERTOS.configGENERATE_RUN_TIME_STATS=1
FREERTOS.configTOTAL_HEAP_SIZE=32768
FREERTOS.configUSE_NEWLIB_REENTRANT=1
FREERTOS.configUSE_TRACE_FACILITY=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C3.I2C_Speed_Mode=I2C_Fast
I2C3.IPParameters=Timing,I2C_Speed_Mode
I2C3.Timing=0x6000030D
KeepUserPlacement=false
Mcu.CPN=STM32F723IEK6
Mcu.Family=STM32F7
Mcu.IP0=CORTEX_M7
Mcu.IP1=FMC
Mcu.IP2=FREERTOS
Mcu.IP3=I2C3
Mcu.IP4=NVIC
Mcu.IP5=RCC
Mcu.IP6=SYS
Mcu.IP7=USART6
Mcu.IPNb=8
Mcu.Name=STM32F723I(C-E)Kx
Mcu.Package=UFBGA176
Mcu.Pin0=PE3
Mcu.Pin1=PE2
Mcu.Pin10=PD7
Mcu.Pin100=PG0
Mcu.Pin101=PE13
Mcu.Pin102=PH7
Mcu.Pin103=PD12
Mcu.Pin104=PD11
Mcu.Pin105=PD10
Mcu.Pin106=PA2
Mcu.Pin107=PA6
Mcu.Pin108=PA5
Mcu.Pin109=PC5
Mcu.Pin11=PC12
Mcu.Pin110=PF12
Mcu.Pin111=PF15
Mcu.Pin112=PE8
Mcu.Pin113=PE9
Mcu.Pin114=PE11
Mcu.Pin115=PE14
Mcu.Pin116=PB12
Mcu.Pin117=PB13
Mcu.Pin118=PD9
Mcu.Pin119=PD8
Mcu.Pin12=PA15
Mcu.Pin120=PA3
Mcu.Pin121=PA7
Mcu.Pin122=PB1
Mcu.Pin123=PB0
Mcu.Pin124=PF11
Mcu.Pin125=PF14
Mcu.Pin126=PE7
Mcu.Pin127=PE10
Mcu.Pin128=PE12
Mcu.Pin129=PE15
Mcu.Pin13=PA14
Mcu.Pin130=PB10
Mcu.Pin131=PB11
Mcu.Pin132=PB14
Mcu.Pin133=PB15
Mcu.Pin134=VP_FREERTOS_VS_CMSIS_V1
Mcu.Pin135=VP_SYS_VS_tim14
Mcu.Pin14=PA13
Mcu.Pin15=PE4
Mcu.Pin16=PE5
Mcu.Pin17=PE6
Mcu.Pin18=PB9
Mcu.Pin19=PB7
Mcu.Pin2=PE1
Mcu.Pin20=PB6
Mcu.Pin21=PG15
Mcu.Pin22=PG12
Mcu.Pin23=PG10
Mcu.Pin24=PD6
Mcu.Pin25=PD0
Mcu.Pin26=PC11
Mcu.Pin27=PC10
Mcu.Pin28=PA12
Mcu.Pin29=PI7
Mcu.Pin3=PE0
Mcu.Pin30=PI6
Mcu.Pin31=PI5
Mcu.Pin32=PG9
Mcu.Pin33=PD5
Mcu.Pin34=PD1
Mcu.Pin35=PI3
Mcu.Pin36=PI2
Mcu.Pin37=PA11
Mcu.Pin38=PI9
Mcu.Pin39=PI4
Mcu.Pin4=PB8
Mcu.Pin40=PD4
Mcu.Pin41=PD3
Mcu.Pin42=PD2
Mcu.Pin43=PH15
Mcu.Pin44=PI1
Mcu.Pin45=PA10
Mcu.Pin46=PC14-OSC32_IN
Mcu.Pin47=PF0
Mcu.Pin48=PI10
Mcu.Pin49=PH13
Mcu.Pin5=PB5
Mcu.Pin50=PH14
Mcu.Pin51=PI0
Mcu.Pin52=PA9
Mcu.Pin53=PC15-OSC32_OUT
Mcu.Pin54=PH2
Mcu.Pin55=PC9
Mcu.Pin56=PA8
Mcu.Pin57=PH0-OSC_IN
Mcu.Pin58=PH3
Mcu.Pin59=PC8
Mcu.Pin6=PG14
Mcu.Pin60=PC7
Mcu.Pin61=PH1-OSC_OUT
Mcu.Pin62=PF2
Mcu.Pin63=PF1
Mcu.Pin64=PH4
Mcu.Pin65=PG8
Mcu.Pin66=PC6
Mcu.Pin67=PF3
Mcu.Pin68=PF4
Mcu.Pin69=PH5
Mcu.Pin7=PG13
Mcu.Pin70=PF7
Mcu.Pin71=PF6
Mcu.Pin72=PF5
Mcu.Pin73=PH12
Mcu.Pin74=PG5
Mcu.Pin75=PG4
Mcu.Pin76=PG3
Mcu.Pin77=PF10
Mcu.Pin78=PF9
Mcu.Pin79=PF8
Mcu.Pin8=PB4
Mcu.Pin80=PH11
Mcu.Pin81=PH10
Mcu.Pin82=PD15
Mcu.Pin83=PG2
Mcu.Pin84=PC0
Mcu.Pin85=PC1
Mcu.Pin86=PC2
Mcu.Pin87=PC3
Mcu.Pin88=PB2
Mcu.Pin89=PG1
Mcu.Pin9=PB3
Mcu.Pin90=PH6
Mcu.Pin91=PH8
Mcu.Pin92=PH9
Mcu.Pin93=PD14
Mcu.Pin94=PD13
Mcu.Pin95=PA1
Mcu.Pin96=PA0-WKUP
Mcu.Pin97=PA4
Mcu.Pin98=PC4
Mcu.Pin99=PF13
Mcu.PinsNb=136
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32F723IEKx
MxCube.Version=6.15.0
MxDb.Version=DB.6.0.150
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:true\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:true\:true\:false
NVIC.TIM8_TRG_COM_TIM14_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM8_TRG_COM_TIM14_IRQn
NVIC.TimeBaseIP=TIM14
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false\:false
PA0-WKUP.Locked=true
PA0-WKUP.Signal=GPIO_Input
PA1.GPIOParameters=GPIO_Label
PA1.GPIO_Label=ARD_D10_TIM2_CH2_SPI1_NSS
PA1.Locked=true
PA1.Signal=S_TIM2_CH2
PA10.GPIOParameters=GPIO_Label
PA10.GPIO_Label=USB_OTG_FS_ID
PA10.Locked=true
PA10.Signal=GPIO_Output
PA11.Locked=true
PA11.Signal=USB_OTG_FS_DM
PA12.Locked=true
PA12.Signal=USB_OTG_FS_DP
PA13.Locked=true
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.Locked=true
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA15.GPIOParameters=GPIO_Label
PA15.GPIO_Label=STMOD_TIM2_CH1_2_ETR
PA15.Locked=true
PA15.Signal=S_TIM2_CH1_ETR
PA2.GPIOParameters=GPIO_Label
PA2.GPIO_Label=ARD_D1_USART2_TX
PA2.Locked=true
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=ARD_D0_USART2_RX
PA3.Locked=true
PA3.Signal=USART2_RX
PA4.GPIOParameters=GPIO_Label
PA4.GPIO_Label=ARD_A1
PA4.Locked=true
PA4.Signal=ADCx_IN4
PA5.Locked=true
PA5.Signal=GPIO_Output
PA6.GPIOParameters=GPIO_Label
PA6.GPIO_Label=ARD_A0
PA6.Locked=true
PA6.Signal=ADCx_IN6
PA7.GPIOParameters=GPIO_Label
PA7.GPIO_Label=SYS_LD_USER1
PA7.Locked=true
PA7.Signal=GPIO_Output
PA8.GPIOParameters=GPIO_Label
PA8.GPIO_Label=CTP_SCL
PA8.Locked=true
PA8.Mode=I2C
PA8.Signal=I2C3_SCL
PA9.Locked=true
PA9.Signal=USB_OTG_FS_VBUS
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=ARD_D5_STMOD_TIM3_CH3
PB0.Locked=true
PB0.Signal=S_TIM3_CH3
PB1.GPIOParameters=GPIO_Label
PB1.GPIO_Label=SYS_LD_USER2
PB1.Locked=true
PB1.Signal=GPIO_Output
PB10.GPIOParameters=GPIO_Label
PB10.GPIO_Label=USB_OTGFS_OVCR_INT
PB10.Locked=true
PB10.Signal=GPXTI10
PB11.GPIOParameters=GPIO_Label
PB11.GPIO_Label=PMOD_INT
PB11.Locked=true
PB11.Signal=GPXTI11
PB12.GPIOParameters=GPIO_Label
PB12.GPIO_Label=USB_OTG_HS_ID
PB12.Locked=true
PB12.Signal=GPIO_Output
PB13.GPIOParameters=GPIO_Label
PB13.GPIO_Label=USB_OTG_HS_VBUS
PB13.Locked=true
PB13.Signal=GPXTI13
PB14.Locked=true
PB14.Signal=USB_OTG_HS_DM
PB15.Locked=true
PB15.Signal=USB_OTG_HS_DP
PB2.GPIOParameters=GPIO_Label
PB2.GPIO_Label=QSPI_CLK [MX25L51245G_SCLK]
PB2.Locked=true
PB2.Signal=QUADSPI_CLK
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=SYS_STLINK_JTDO_SWO
PB3.Locked=true
PB3.Signal=SYS_JTDO-SWO
PB4.GPIOParameters=GPIO_Label
PB4.GPIO_Label=ARD_D12_SPI1_MISO
PB4.Locked=true
PB4.Signal=SPI1_MISO
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=ARD_D11_TIM3_CH2_SPI1_MOSI
PB5.Locked=true
PB5.Signal=SPI1_MOSI
PB6.GPIOParameters=GPIO_Label
PB6.GPIO_Label=QSPI_NCS [MX25L51245G_CS]
PB6.Locked=true
PB6.Signal=QUADSPI_BK1_NCS
PB7.GPIOParameters=GPIO_Label
PB7.GPIO_Label=NC1
PB7.Locked=true
PB7.Signal=FMC_NL
PB8.GPIOParameters=GPIO_Label
PB8.GPIO_Label=SAI2_I2C1_SCL [WM8994ECS/R_SCLK]
PB8.Locked=true
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Label
PB9.GPIO_Label=SAI2_I2C1_SDA [WM8994ECS_SDA]
PB9.Locked=true
PB9.Signal=I2C1_SDA
PC0.GPIOParameters=GPIO_Label
PC0.GPIO_Label=ARD_A4
PC0.Locked=true
PC0.Signal=ADCx_IN10
PC1.GPIOParameters=GPIO_Label
PC1.GPIO_Label=ARD_A5
PC1.Locked=true
PC1.Signal=ADCx_IN11
PC10.GPIOParameters=GPIO_Label
PC10.GPIO_Label=QSPI_D1 [MX25L51245G_SIO1]
PC10.Locked=true
PC10.Signal=QUADSPI_BK1_IO1
PC11.GPIOParameters=GPIO_Label
PC11.GPIO_Label=STMOD_UART4_RXD_s
PC11.Locked=true
PC11.Signal=GPIO_Output
PC12.GPIOParameters=GPIO_Label
PC12.GPIO_Label=UART_TXD_WIFI_RX
PC12.Locked=true
PC12.Signal=UART5_TX
PC14-OSC32_IN.Locked=true
PC14-OSC32_IN.Mode=LSE-External-Oscillator
PC14-OSC32_IN.Signal=RCC_OSC32_IN
PC15-OSC32_OUT.Locked=true
PC15-OSC32_OUT.Mode=LSE-External-Oscillator
PC15-OSC32_OUT.Signal=RCC_OSC32_OUT
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=STMOD_SPI2_MISOs
PC2.Locked=true
PC2.Signal=SPI2_MISO
PC3.GPIOParameters=GPIO_Label
PC3.GPIO_Label=STMOD_SPI2_MOSIs
PC3.Locked=true
PC3.Signal=SPI2_MOSI
PC4.GPIOParameters=GPIO_Label
PC4.GPIO_Label=ARD_A2
PC4.Locked=true
PC4.Signal=ADCx_IN14
PC5.GPIOParameters=GPIO_Label
PC5.GPIO_Label=ARD_D2_GPIO
PC5.Locked=true
PC5.Signal=GPIO_Output
PC6.GPIOParameters=GPIO_Label
PC6.GPIO_Label=VCP_TX [STM32F103CBT6_PA3]
PC6.Locked=true
PC6.Mode=Asynchronous
PC6.Signal=USART6_TX
PC7.GPIOParameters=GPIO_Label
PC7.GPIO_Label=VCP_RX [STM32F103CBT6_PA2]
PC7.Locked=true
PC7.Mode=Asynchronous
PC7.Signal=USART6_RX
PC8.GPIOParameters=GPIO_Label
PC8.GPIO_Label=LCD_TE_INT
PC8.Locked=true
PC8.Signal=GPXTI8
PC9.GPIOParameters=GPIO_Label
PC9.GPIO_Label=QSPI_D0 [MX25L51245G_SIO0]
PC9.Locked=true
PC9.Signal=QUADSPI_BK1_IO0
PD0.GPIOParameters=GPIO_Label
PD0.GPIO_Label=LCD_PSRAM_D2
PD0.Locked=true
PD0.Signal=FMC_D2_DA2
PD1.GPIOParameters=GPIO_Label
PD1.GPIO_Label=LCD_PSRAM_D3
PD1.Locked=true
PD1.Signal=FMC_D3_DA3
PD10.GPIOParameters=GPIO_Label
PD10.GPIO_Label=LCD_PSRAM_D15
PD10.Locked=true
PD10.Signal=FMC_D15_DA15
PD11.GPIOParameters=GPIO_Label
PD11.GPIO_Label=PSRAM_A16
PD11.Locked=true
PD11.Signal=FMC_A16_CLE
PD12.GPIOParameters=GPIO_Label
PD12.GPIO_Label=PSRAM_A17
PD12.Locked=true
PD12.Signal=FMC_A17_ALE
PD13.GPIOParameters=GPIO_Label
PD13.GPIO_Label=QSPI_D3 [MX25L51245G_SIO3]
PD13.Locked=true
PD13.Signal=QUADSPI_BK1_IO3
PD14.GPIOParameters=GPIO_Label
PD14.GPIO_Label=LCD_PSRAM_D0
PD14.Locked=true
PD14.Signal=FMC_D0_DA0
PD15.GPIOParameters=GPIO_Label
PD15.GPIO_Label=LCD_PSRAM_D1
PD15.Locked=true
PD15.Signal=FMC_D1_DA1
PD2.GPIOParameters=GPIO_Label
PD2.GPIO_Label=UART_RXD_WIFI_TX
PD2.Locked=true
PD2.Signal=UART5_RX
PD3.GPIOParameters=GPIO_Label
PD3.GPIO_Label=WIFI_CH_PD
PD3.Locked=true
PD3.Signal=GPIO_Output
PD4.GPIOParameters=GPIO_Label
PD4.GPIO_Label=LCD_PSRAM_NWE
PD4.Locked=true
PD4.Signal=FMC_NOE
PD5.GPIOParameters=GPIO_Label
PD5.GPIO_Label=LCD_PSRAM_NWE
PD5.Locked=true
PD5.Signal=FMC_NWE
PD6.GPIOParameters=GPIO_Label
PD6.GPIO_Label=WIFI_GPIO_2
PD6.Locked=true
PD6.Signal=GPIO_Output
PD7.GPIOParameters=GPIO_Label
PD7.GPIO_Label=PSRAM_NE1 [IS66WV51216EBLL_CS1]
PD7.Locked=true
PD7.Signal=FMC_NE1
PD8.GPIOParameters=GPIO_Label
PD8.GPIO_Label=LCD_PSRAM_D13
PD8.Locked=true
PD8.Signal=FMC_D13_DA13
PD9.GPIOParameters=GPIO_Label
PD9.GPIO_Label=LCD_PSRAM_D14
PD9.Locked=true
PD9.Signal=FMC_D14_DA14
PE0.GPIOParameters=GPIO_Label
PE0.GPIO_Label=PSRAM_NBL0 [IS66WV51216EBLL_LB]
PE0.Locked=true
PE0.Signal=FMC_NBL0
PE1.GPIOParameters=GPIO_Label
PE1.GPIO_Label=PSRAM_NBL1 [IS66WV51216EBLL_UB]
PE1.Locked=true
PE1.Signal=FMC_NBL1
PE10.GPIOParameters=GPIO_Label
PE10.GPIO_Label=LCD_PSRAM_D7
PE10.Locked=true
PE10.Signal=FMC_D7_DA7
PE11.GPIOParameters=GPIO_Label
PE11.GPIO_Label=LCD_PSRAM_D8
PE11.Locked=true
PE11.Signal=FMC_D8_DA8
PE12.GPIOParameters=GPIO_Label
PE12.GPIO_Label=LCD_PSRAM_D9
PE12.Locked=true
PE12.Signal=FMC_D9_DA9
PE13.GPIOParameters=GPIO_Label
PE13.GPIO_Label=LCD_PSRAM_D10
PE13.Locked=true
PE13.Signal=FMC_D10_DA10
PE14.GPIOParameters=GPIO_Label
PE14.GPIO_Label=LCD_PSRAM_D11
PE14.Locked=true
PE14.Signal=FMC_D11_DA11
PE15.GPIOParameters=GPIO_Label
PE15.GPIO_Label=LCD_PSRAM_D12
PE15.Locked=true
PE15.Signal=FMC_D12_DA12
PE2.GPIOParameters=GPIO_Label
PE2.GPIO_Label=QSPI_D2 [MX25L51245G_SIO2]
PE2.Locked=true
PE2.Signal=QUADSPI_BK1_IO2
PE3.GPIOParameters=GPIO_Label
PE3.GPIO_Label=ARD_D7_GPIO
PE3.Locked=true
PE3.Signal=GPIO_Output
PE4.GPIOParameters=GPIO_Label
PE4.GPIO_Label=ARD_D8_GPIO
PE4.Locked=true
PE4.Signal=GPIO_Output
PE5.GPIOParameters=GPIO_Label
PE5.GPIO_Label=ARD_D3_TIM9_CH1
PE5.Locked=true
PE5.Signal=S_TIM9_CH1
PE6.GPIOParameters=GPIO_Label
PE6.GPIO_Label=ARD_D6_TIM9_CH2
PE6.Locked=true
PE6.Signal=S_TIM9_CH2
PE7.GPIOParameters=GPIO_Label
PE7.GPIO_Label=LCD_PSRAM_D4
PE7.Locked=true
PE7.Signal=FMC_D4_DA4
PE8.GPIOParameters=GPIO_Label
PE8.GPIO_Label=LCD_PSRAM_D5
PE8.Locked=true
PE8.Signal=FMC_D5_DA5
PE9.GPIOParameters=GPIO_Label
PE9.GPIO_Label=LCD_PSRAM_D6
PE9.Locked=true
PE9.Signal=FMC_D6_DA6
PF0.GPIOParameters=GPIO_Label
PF0.GPIO_Label=PSRAM_A0
PF0.Locked=true
PF0.Signal=FMC_A0
PF1.GPIOParameters=GPIO_Label
PF1.GPIO_Label=PSRAM_A1
PF1.Locked=true
PF1.Signal=FMC_A1
PF10.GPIOParameters=GPIO_Label
PF10.GPIO_Label=ARD_A3_ADC3_IN8
PF10.Locked=true
PF10.Signal=ADC3_IN8
PF11.GPIOParameters=GPIO_Label
PF11.GPIO_Label=PMOD_RESET
PF11.Locked=true
PF11.Signal=GPIO_Input
PF12.GPIOParameters=GPIO_Label
PF12.GPIO_Label=PSRAM_A6
PF12.Locked=true
PF12.Signal=FMC_A6
PF13.GPIOParameters=GPIO_Label
PF13.GPIO_Label=PSRAM_A7
PF13.Locked=true
PF13.Signal=FMC_A7
PF14.GPIOParameters=GPIO_Label
PF14.GPIO_Label=PSRAM_A8
PF14.Locked=true
PF14.Signal=FMC_A8
PF15.GPIOParameters=GPIO_Label
PF15.GPIO_Label=PSRAM_A9
PF15.Locked=true
PF15.Signal=FMC_A9
PF2.GPIOParameters=GPIO_Label
PF2.GPIO_Label=PSRAM_A2
PF2.Locked=true
PF2.Signal=FMC_A2
PF3.GPIOParameters=GPIO_Label
PF3.GPIO_Label=PSRAM_A3
PF3.Locked=true
PF3.Signal=FMC_A3
PF4.GPIOParameters=GPIO_Label
PF4.GPIO_Label=PSRAM_A4
PF4.Locked=true
PF4.Signal=FMC_A4
PF5.GPIOParameters=GPIO_Label
PF5.GPIO_Label=PSRAM_A5
PF5.Locked=true
PF5.Signal=FMC_A5
PF6.GPIOParameters=GPIO_Label
PF6.GPIO_Label=PMOD_UART7_RXD
PF6.Locked=true
PF6.Signal=UART7_RX
PF7.GPIOParameters=GPIO_Label
PF7.GPIO_Label=PMOD_UART7_TXD
PF7.Locked=true
PF7.Signal=UART7_TX
PF8.GPIOParameters=GPIO_Label
PF8.GPIO_Label=PMOD_UART7_RTS
PF8.Locked=true
PF8.Signal=UART7_RTS
PF9.GPIOParameters=GPIO_Label
PF9.GPIO_Label=PMOD_UART7_CTS
PF9.Locked=true
PF9.Signal=UART7_CTS
PG0.GPIOParameters=GPIO_Label
PG0.GPIO_Label=PSRAM_A10
PG0.Locked=true
PG0.Signal=FMC_A10
PG1.GPIOParameters=GPIO_Label
PG1.GPIO_Label=PSRAM_A11
PG1.Locked=true
PG1.Signal=FMC_A11
PG10.GPIOParameters=GPIO_Label
PG10.GPIO_Label=SAI2_SD_B [SAI2_SD_B_ADCDAT1]
PG10.Locked=true
PG10.Signal=SAI2_SD_B
PG12.GPIOParameters=GPIO_Label
PG12.GPIO_Label=PMOD_GPIO_0
PG12.Locked=true
PG12.Signal=GPIO_Output
PG13.GPIOParameters=GPIO_Label
PG13.GPIO_Label=WIFI_GPIO_0
PG13.Locked=true
PG13.Signal=GPIO_Output
PG14.GPIOParameters=GPIO_Label
PG14.GPIO_Label=WIFI_RST
PG14.Locked=true
PG14.Signal=GPIO_Output
PG15.GPIOParameters=GPIO_Label
PG15.GPIO_Label=SAI2_INT [WM8994ECS_GPIO1]
PG15.Locked=true
PG15.Signal=GPXTI15
PG2.GPIOParameters=GPIO_Label
PG2.GPIO_Label=PSRAM_A12
PG2.Locked=true
PG2.Signal=FMC_A12
PG3.GPIOParameters=GPIO_Label
PG3.GPIO_Label=PSRAM_A13
PG3.Locked=true
PG3.Signal=FMC_A13
PG4.GPIOParameters=GPIO_Label
PG4.GPIO_Label=PSRAM_A14
PG4.Locked=true
PG4.Signal=FMC_A14_BA0
PG5.GPIOParameters=GPIO_Label
PG5.GPIO_Label=PSRAM_A15
PG5.Locked=true
PG5.Signal=FMC_A15_BA1
PG8.GPIOParameters=GPIO_Label
PG8.GPIO_Label=USB_OTGFS_PPWR_EN
PG8.Locked=true
PG8.Signal=GPIO_Output
PG9.GPIOParameters=GPIO_Label
PG9.GPIO_Label=LCD_NE
PG9.Locked=true
PG9.Mode=NorPsramChipSelect2_2
PG9.Signal=FMC_NE2
PH0-OSC_IN.Locked=true
PH0-OSC_IN.Mode=HSE-External-Oscillator
PH0-OSC_IN.Signal=RCC_OSC_IN
PH1-OSC_OUT.Locked=true
PH1-OSC_OUT.Mode=HSE-External-Oscillator
PH1-OSC_OUT.Signal=RCC_OSC_OUT
PH10.GPIOParameters=GPIO_Label
PH10.GPIO_Label=USB_OTGHS_OVCR_INT
PH10.Locked=true
PH10.Signal=GPIO_Input
PH11.Locked=true
PH11.Signal=GPIO_Output
PH12.Locked=true
PH12.Signal=GPIO_Output
PH13.GPIOParameters=GPIO_Label
PH13.GPIO_Label=STMOD_UART4_TXD
PH13.Locked=true
PH13.Signal=UART4_TX
PH14.GPIOParameters=GPIO_Label
PH14.GPIO_Label=STMOD_UART4_RXD
PH14.Locked=true
PH14.Signal=UART4_RX
PH15.GPIOParameters=PinState,GPIO_Label
PH15.GPIO_Label=PMOD_SEL_0
PH15.Locked=true
PH15.PinState=GPIO_PIN_SET
PH15.Signal=GPIO_Output
PH2.GPIOParameters=GPIO_Label
PH2.GPIO_Label=PMOD_GPIO_1
PH2.Locked=true
PH2.Signal=GPIO_Output
PH3.GPIOParameters=GPIO_Label
PH3.GPIO_Label=ARD_D4_GPIO
PH3.Locked=true
PH3.Signal=GPIO_Output
PH4.GPIOParameters=GPIO_Label
PH4.GPIO_Label=ARD_D15_STMOD_I2C2_SCL
PH4.Locked=true
PH4.Signal=I2C2_SCL
PH5.GPIOParameters=GPIO_Label
PH5.GPIO_Label=ARD_D14_STMOD_I2C2_SDA
PH5.Locked=true
PH5.Signal=I2C2_SDA
PH6.GPIOParameters=GPIO_Label
PH6.GPIO_Label=ARD_D9_TIM12_CH1
PH6.Locked=true
PH6.Signal=S_TIM12_CH1
PH7.GPIOParameters=GPIO_Label
PH7.GPIO_Label=LCD_RST
PH7.Locked=true
PH7.Signal=GPIO_Output
PH8.GPIOParameters=GPIO_Label
PH8.GPIO_Label=CTP_SDA
PH8.Locked=true
PH8.Mode=I2C
PH8.Signal=I2C3_SDA
PH9.GPIOParameters=PinState,GPIO_Label
PH9.GPIO_Label=CTP_RST
PH9.Locked=true
PH9.PinState=GPIO_PIN_SET
PH9.Signal=GPIO_Output
PI0.GPIOParameters=GPIO_Label
PI0.GPIO_Label=PMOD_SPI2_NSS
PI0.Locked=true
PI0.Signal=SPI2_NSS
PI1.GPIOParameters=GPIO_Label
PI1.GPIO_Label=PMOD_SPI2_SCK
PI1.Locked=true
PI1.Signal=SPI2_SCK
PI10.Locked=true
PI10.Signal=GPIO_Output
PI2.GPIOParameters=GPIO_Label
PI2.GPIO_Label=PMOD_SPI2_MISO
PI2.Locked=true
PI2.Signal=GPIO_Output
PI3.GPIOParameters=GPIO_Label
PI3.GPIO_Label=PMOD_SPI2_MOSI
PI3.Locked=true
PI3.Signal=GPIO_Output
PI4.GPIOParameters=GPIO_Label
PI4.GPIO_Label=SAI2_MCLK_A [WM8994ECS_MCLK1]
PI4.Locked=true
PI4.Signal=SAI2_MCLK_A
PI5.GPIOParameters=GPIO_Label
PI5.GPIO_Label=SAI2_SCK_A [WM8994ECS_BCLK1]
PI5.Locked=true
PI5.Signal=SAI2_SCK_A
PI6.GPIOParameters=GPIO_Label
PI6.GPIO_Label=SAI2_SD_A [WM8994ECS_DACDAT1]
PI6.Locked=true
PI6.Signal=SAI2_SD_A
PI7.GPIOParameters=GPIO_Label
PI7.GPIO_Label=SAI2_FS_A [WM8994ECS_LRCLK1]
PI7.Locked=true
PI7.Signal=SAI2_FS_A
PI9.GPIOParameters=GPIO_Label
PI9.GPIO_Label=CTP_INT
PI9.Locked=true
PI9.Signal=GPXTI9
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerLinker=GCC
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F723IEKx
ProjectManager.FirmwarePackage=STM32Cube FW_F7 V1.17.4
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=Versuch3.ioc
ProjectManager.ProjectName=Versuch3
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_USART6_UART_Init-USART6-false-HAL-true,4-MX_FMC_Init-FMC-false-HAL-true,5-MX_I2C3_Init-I2C3-false-HAL-true,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
RCC.AHBFreq_Value=216000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=54000000
RCC.APB1TimFreq_Value=108000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=108000000
RCC.APB2TimFreq_Value=216000000
RCC.CortexFreq_Value=216000000
RCC.FCLKCortexFreq_Value=216000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=216000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=54000000
RCC.I2C2Freq_Value=54000000
RCC.I2C3Freq_Value=54000000
RCC.I2SFreq_Value=96000000
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CortexFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2SFreq_Value,LPTIM1Freq_Value,LSI_VALUE,MCO2PinFreq_Value,PLLCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SRoutputFreq_Value,PLLM,PLLN,PLLQ,PLLQCLKFreq_Value,PLLQoutputFreq_Value,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIoutputFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMC2Freq_Value,SDMMCFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,UART7Freq_Value,UART8Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value
RCC.LPTIM1Freq_Value=54000000
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=216000000
RCC.PLLCLKFreq_Value=216000000
RCC.PLLI2SQCLKFreq_Value=96000000
RCC.PLLI2SRCLKFreq_Value=96000000
RCC.PLLI2SRoutputFreq_Value=96000000
RCC.PLLM=25
RCC.PLLN=432
RCC.PLLQ=9
RCC.PLLQCLKFreq_Value=48000000
RCC.PLLQoutputFreq_Value=48000000
RCC.PLLSAIPCLKFreq_Value=96000000
RCC.PLLSAIQCLKFreq_Value=96000000
RCC.PLLSAIoutputFreq_Value=96000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=48000000
RCC.SAI1Freq_Value=96000000
RCC.SAI2Freq_Value=96000000
RCC.SDMMC2Freq_Value=216000000
RCC.SDMMCFreq_Value=216000000
RCC.SYSCLKFreq_VALUE=216000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=54000000
RCC.UART5Freq_Value=54000000
RCC.UART7Freq_Value=54000000
RCC.UART8Freq_Value=54000000
RCC.USART1Freq_Value=108000000
RCC.USART2Freq_Value=54000000
RCC.USART3Freq_Value=54000000
RCC.USART6Freq_Value=108000000
RCC.USBFreq_Value=48000000
RCC.VCOI2SOutputFreq_Value=192000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=432000000
RCC.VCOSAIOutputFreq_Value=192000000
SH.ADCx_IN10.0=ADC2_IN10
SH.ADCx_IN10.ConfNb=1
SH.ADCx_IN11.0=ADC2_IN11
SH.ADCx_IN11.ConfNb=1
SH.ADCx_IN14.0=ADC2_IN14
SH.ADCx_IN14.ConfNb=1
SH.ADCx_IN4.0=ADC2_IN4
SH.ADCx_IN4.ConfNb=1
SH.ADCx_IN6.0=ADC2_IN6
SH.ADCx_IN6.ConfNb=1
SH.FMC_A0.0=FMC_A0,A0_2
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11
SH.FMC_A11.ConfNb=1
SH.FMC_A12.0=FMC_A12
SH.FMC_A12.ConfNb=1
SH.FMC_A13.0=FMC_A13
SH.FMC_A13.ConfNb=1
SH.FMC_A14_BA0.0=FMC_A14
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_A15
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A16_CLE.0=FMC_A16
SH.FMC_A16_CLE.ConfNb=1
SH.FMC_A17_ALE.0=FMC_A17
SH.FMC_A17_ALE.ConfNb=1
SH.FMC_A2.0=FMC_A2
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,16b-d2
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,16b-d2
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,16b-d2
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,16b-d2
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,16b-d2
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,16b-d2
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,16b-d2
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,16b-d2
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,16b-d2
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,16b-d2
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,16b-d2
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,16b-d2
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,16b-d2
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,16b-d2
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,16b-d2
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,16b-d2
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1
SH.FMC_NBL1.ConfNb=1
SH.FMC_NL.0=FMC_NL
SH.FMC_NL.ConfNb=1
SH.FMC_NOE.0=FMC_NOE,Lcd2
SH.FMC_NOE.ConfNb=1
SH.FMC_NWE.0=FMC_NWE,Lcd2
SH.FMC_NWE.ConfNb=1
SH.GPXTI10.0=GPIO_EXTI10
SH.GPXTI10.ConfNb=1
SH.GPXTI11.0=GPIO_EXTI11
SH.GPXTI11.ConfNb=1
SH.GPXTI13.0=GPIO_EXTI13
SH.GPXTI13.ConfNb=1
SH.GPXTI15.0=GPIO_EXTI15
SH.GPXTI15.ConfNb=1
SH.GPXTI8.0=GPIO_EXTI8
SH.GPXTI8.ConfNb=1
SH.GPXTI9.0=GPIO_EXTI9
SH.GPXTI9.ConfNb=1
SH.S_TIM12_CH1.0=TIM12_CH1
SH.S_TIM12_CH1.ConfNb=1
SH.S_TIM2_CH1_ETR.0=TIM2_CH1
SH.S_TIM2_CH1_ETR.ConfNb=1
SH.S_TIM2_CH2.0=TIM2_CH2
SH.S_TIM2_CH2.ConfNb=1
SH.S_TIM3_CH3.0=TIM3_CH3
SH.S_TIM3_CH3.ConfNb=1
SH.S_TIM9_CH1.0=TIM9_CH1
SH.S_TIM9_CH1.ConfNb=1
SH.S_TIM9_CH2.0=TIM9_CH2
SH.S_TIM9_CH2.ConfNb=1
USART6.IPParameters=VirtualMode-Asynchronous
USART6.VirtualMode-Asynchronous=VM_ASYNC
VP_FREERTOS_VS_CMSIS_V1.Mode=CMSIS_V1
VP_FREERTOS_VS_CMSIS_V1.Signal=FREERTOS_VS_CMSIS_V1
VP_SYS_VS_tim14.Mode=TIM14
VP_SYS_VS_tim14.Signal=SYS_VS_tim14
board=STM32F723E-DISCO
boardIOC=true
rtos.0.ip=FREERTOS
isbadioc=false
