# Notes about milling pcb led-boards_v0.1
**2024.11.17:**
- used 60 degree big (0.2mm depth)
- center bridge broke off and pcb went up **-> make bridges longer / more solid** (pcb uneven)
- mount screws of 8x leds can not be used, to close to outline -> drilled separate mounting holes outside


# notes about kicad export (general)
- dont tick "use gerber X2 format (recommended)" to prevent many unsupported warnings
- dont tick unnecessary plot xx options e.g. "plot footprint text" it might cause hangup
- if oval holes are present select "Use alternative drill mode" option in generate drill files menu