(footprint "WAGO 734-164 Print-Stiftleiste, Mini, RM 3,5, gewinkelt, 4-polig"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "6dc14bdf-ecc5-40ff-a50e-8abd42383bcc")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "WAGO 734-164 Print-Stiftleiste, Mini, RM 3,5, gewinkelt, 4-polig"
		(at 9.5 10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "50b26567-c223-4790-b859-0af598207a87")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "877c3506-ed90-43f1-847c-d051415b93ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f64a93cc-c27b-4699-a4b7-0cb6a7991177")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9168185a-c961-46e4-92b6-fa7617d2cba7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 0 8)
		(end 0 5.5)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "35b38eaa-361c-4f67-a905-71eec74e4b44")
	)
	(fp_line
		(start 3.5 8)
		(end 3.5 5.5)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c1d58c63-b685-4eee-aa3b-7ca9eed66f14")
	)
	(fp_line
		(start 7 8)
		(end 7 5.5)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "63e40b59-13f4-4f47-84d4-57ba377069ae")
	)
	(fp_line
		(start 10.5 8)
		(end 10.5 5.5)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "329ab3dc-1f3b-436c-9ce9-29685c72f487")
	)
	(fp_rect
		(start -2.8 -1)
		(end 13.3 9.3)
		(stroke
			(width 0.25)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "2b6efbf7-69a4-4da9-af42-cb2af2ae55eb")
	)
	(fp_rect
		(start -1.9 5.5)
		(end 12.4 9.3)
		(stroke
			(width 0.25)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "034318e1-73d6-4339-b64b-b44c8b06fe1d")
	)
	(fp_rect
		(start -3.5 -1.5)
		(end 14 10)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "d12c9877-f04e-403d-9c45-f826a9c07833")
	)
	(fp_text user "${REFERENCE}"
		(at 12.5 3.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4fa21bca-afe7-40d0-8881-c6a1b018d0dd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 2.8 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d15eb621-bcba-48ab-bb37-6da8bcf2d82e")
	)
	(pad "2" thru_hole oval
		(at 3.5 0)
		(size 2.8 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bee68793-bfbb-4908-b67a-c79cc14550a3")
	)
	(pad "3" thru_hole oval
		(at 7 0)
		(size 2.8 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5e7c8131-156c-454b-89c2-e6f78d23a3dc")
	)
	(pad "4" thru_hole oval
		(at 10.5 0)
		(size 2.8 3.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f4ebbed4-1bed-474b-ade9-3bc405da8a30")
	)
	(model "U:/IO-Adapter/custom-kicad-library/3d-models/Wago_734-164_1x04_P3.50mm_Horizontal.stp"
		(offset
			(xyz 13.6 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
