(footprint "WAGO 736-306 Doppelstockklemme 2.50 mm2 Polzahl 12"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -17.8 7.2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "748bfa7a-63ee-4685-b60e-abf0eb47e44f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "WAGO 736-306 Doppelstockklemme 2.50 mm2 Polzahl 12"
		(at -5.4 12.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1bad0c2b-dc00-4b70-a45f-aa648b0c2463")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -17.8 7.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0b8e98b4-1060-4c5e-9793-180af9aee5a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -17.8 7.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d3e65c66-0de0-49df-bb4d-0ff433a0193a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -17.8 7.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8e3844a9-7810-40a8-9823-7927da60595b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -20.8 -9.56)
		(end 10.5 11.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "3c21acfa-9df2-43ea-ac44-91eee4acdfc2")
	)
	(fp_rect
		(start -19.07 -5)
		(end -16.53 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "af04f3de-c200-4cce-b7a0-6782b1b723c1")
	)
	(fp_rect
		(start -19.07 1.35)
		(end -16.53 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "367cfc37-f6c2-4990-ad20-e4816cb8a129")
	)
	(fp_rect
		(start -13.99 -5)
		(end -11.45 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "6e9cf488-53fa-4e83-a208-c6b148439c56")
	)
	(fp_rect
		(start -13.99 1.35)
		(end -11.45 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "56314ea4-0de0-4a8f-8794-048541712a58")
	)
	(fp_rect
		(start -8.91 -5)
		(end -6.37 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "cb7e8d12-1bb5-477f-99bf-997da427c84c")
	)
	(fp_rect
		(start -8.91 1.35)
		(end -6.37 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "801cf84c-eb0e-446c-ae01-a41544817e2e")
	)
	(fp_rect
		(start -3.83 -5)
		(end -1.29 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "fb6f6d72-1144-444f-a025-f530bc05577c")
	)
	(fp_rect
		(start -3.83 1.35)
		(end -1.29 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "df9caa05-538d-420b-bb88-bec461d1b820")
	)
	(fp_rect
		(start 1.25 -5)
		(end 3.79 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "c9f2e36c-848c-4153-894c-dd88e91b7567")
	)
	(fp_rect
		(start 1.25 1.35)
		(end 3.79 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e9a16428-16ef-4fbb-b173-9a51ba354822")
	)
	(fp_rect
		(start 6.33 -5)
		(end 8.87 -1.19)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "34c90f11-afad-4f50-86ed-daaf1c6eb7f4")
	)
	(fp_rect
		(start 6.33 1.35)
		(end 8.87 5.16)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "d162b4cd-ee14-49df-82e0-2f23b4f44763")
	)
	(fp_text user "pcb-side"
		(at -8.8 -10.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7c88a11f-d049-4d05-9637-48c7c502cefe")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "calbes-side"
		(at -9.1 11.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e78f45cc-4138-4e59-b827-aeddbc038728")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at -6.1 14.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "59f2633a-fc3b-4b71-8f19-61d05251451d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at -17.8 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "687de134-7c04-4a96-b86f-933a3e792757")
	)
	(pad "2" thru_hole oval
		(at -12.72 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ac2f9f8d-f5c2-4169-8f83-3bea49001f48")
	)
	(pad "3" thru_hole oval
		(at -7.64 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cf3b022a-bfc9-40b4-bd03-4de260e72bea")
	)
	(pad "4" thru_hole oval
		(at -2.56 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6ebd49b0-b2bd-4e4b-9402-844c4b5f8d40")
	)
	(pad "5" thru_hole oval
		(at 2.52 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3450cad1-05e2-4011-8eb4-6e4e024db50f")
	)
	(pad "6" thru_hole oval
		(at 7.6 7.7)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "806c8fa6-e89c-431f-b217-bcca75896891")
	)
	(pad "7" thru_hole oval
		(at -17.78 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a210f080-16a2-4892-8b61-2994d62c2c96")
	)
	(pad "8" thru_hole oval
		(at -12.7 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d5b6163-fa7f-442f-b641-c6f8e186f27c")
	)
	(pad "9" thru_hole oval
		(at -7.62 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d03bfdf9-6324-411c-9a04-9d20b3c40d94")
	)
	(pad "10" thru_hole oval
		(at -2.54 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "68becd1a-8252-4022-a3e7-cac045131f20")
	)
	(pad "11" thru_hole oval
		(at 2.54 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e9ccb96f-0011-472b-ade1-46d951828cbf")
	)
	(pad "12" thru_hole oval
		(at 7.62 -7.62)
		(size 3.5 4.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e8496aa1-fada-4f1b-b206-68c91ad1db98")
	)
	(model "U:/IO-Adapter/custom-kicad-library/3d-models/WAGO 736-306 Doppelstockklemme 2.50 mm2 Polzahl 12.stp"
		(offset
			(xyz 9.5 7.5 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
