(footprint "WAGO 231-533 Print-Stiftleiste, Midi, RM 5,08, gewinkelt, 3-polig"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.508 9.525 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b5c70de4-f490-4841-908c-007ed8c0209a")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "WAGO 231-533 Print-Stiftleiste, Midi, RM 5,08, gewinkelt, 3-polig"
		(at 1.778 6.731 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ebab2512-97bf-4ea4-bdf2-ac3d5dcdbae3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -5.08 -4.445 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcbda2c9-b68d-4fdd-a05f-6be3d9ac47af")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -5.08 -4.445 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c9d8b5fe-6e11-412f-a9bb-9fcfef8a93f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -5.08 -4.445 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c74f356a-21c5-44fd-8d58-dba5b3887a65")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -9.28 -6.445)
		(end 9.32 5.555)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "9916b3fa-9deb-44a0-8193-a81c594ccad1")
	)
	(fp_rect
		(start -6.35 0)
		(end -3.81 3.81)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "66bfc842-9c1f-4090-85b8-8ac36a68144c")
	)
	(fp_rect
		(start -1.27 0)
		(end 1.27 3.81)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "4a48badb-6b59-49a4-83a4-6d4a04fe61fa")
	)
	(fp_rect
		(start 3.81 0)
		(end 6.35 3.81)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "fc069869-dd0f-4be9-8aec-d2c79ec9e48f")
	)
	(fp_text user "${REFERENCE}"
		(at -0.508 8.255 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "97aefc99-3b0d-45b3-830b-343721838759")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at -5.08 -4.445)
		(size 3 4)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "35bae143-abf5-4623-b9e7-39c37a0d85ba")
	)
	(pad "2" thru_hole oval
		(at 0 -4.445)
		(size 3 4)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "651568d8-fa19-4e3c-ad8b-b295dfd15053")
	)
	(pad "3" thru_hole oval
		(at 5.08 -4.445)
		(size 3 4)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b752b56f-55c2-4265-a409-d2c7285b57f7")
	)
	(model "U:/IO-Adapter/custom-kicad-library/3d-models/WAGO 231-533 Print-Stiftleiste, Midi, RM 5,08, gewinkelt, 3-polig.stp"
		(offset
			(xyz 9.17 4.445 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
