# Notes about milling pcb power-supply-board_v1.0
**2024.11.17:**
- used 45 degree big (~0.3mm depth)
- worked well at first but needed full second pass because it did not mill last area (uneven or bit got shorter)
    - next time do 2 passes (smaller depth) with new bit so it does not wear down that fast?


# notes about kicad export (general)
- dont tick "use gerber X2 format (recommended)" to prevent many unsupported warnings
- dont tick unnecessary plot xx options e.g. "plot footprint text" it might cause hangup
- if oval holes are present select "Use alternative drill mode" option in generate drill files menu