(footprint "WAGO 733-366 Print-Stiftleiste, Micro, RM 2,5, gewinkelt, 6-pol"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 2.5 3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "6dc14bdf-ecc5-40ff-a50e-8abd42383bcc")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "WAGO 733-366 Print-Stiftleiste, Micro, RM 2,5, gewinkelt, 6-pol"
		(at 9 12 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "50b26567-c223-4790-b859-0af598207a87")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "877c3506-ed90-43f1-847c-d051415b93ce")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f64a93cc-c27b-4699-a4b7-0cb6a7991177")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9168185a-c961-46e4-92b6-fa7617d2cba7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 2.5 8.25)
		(end 2.5 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "381457a6-2812-4e8a-bdab-7acefa15b43f")
	)
	(fp_line
		(start 5 8.25)
		(end 5 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6dc8f725-024a-457e-ac00-2dd23a76d42b")
	)
	(fp_line
		(start 7.5 8.25)
		(end 7.5 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6a8ff19c-640a-4612-90fd-57686eca25cc")
	)
	(fp_line
		(start 10 8.25)
		(end 10 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "88fd2f6c-1d43-4eb3-9dba-34cf632d48fb")
	)
	(fp_line
		(start 12.5 8.25)
		(end 12.5 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "11b6369a-ba00-4a66-8cac-5e71befe0266")
	)
	(fp_line
		(start 15 8.25)
		(end 15 5.75)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "71ed852a-09d9-4fe0-b038-ea2c0d6fb267")
	)
	(fp_rect
		(start 0 0)
		(end 17.5 9.5)
		(stroke
			(width 0.25)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "540ff40d-f133-43a1-9f97-283c8f220c8f")
	)
	(fp_rect
		(start 1.1 5.75)
		(end 16.4 9.55)
		(stroke
			(width 0.25)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "dbc34783-df6a-4158-9fbd-a31c61ff4347")
	)
	(fp_rect
		(start -0.5 -0.5)
		(end 18 10)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "c7fa08c1-ff34-40bf-b5b9-3581e6a0d67d")
	)
	(fp_text user "${REFERENCE}"
		(at 5 -2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d3635e35-e36e-4b2c-a7b0-23cf22b4cbca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at 2.5 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "be7bea35-2178-45b0-9b8b-cef6f0babf10")
	)
	(pad "2" thru_hole oval
		(at 5 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4a1fecde-ba87-4b11-972d-bddfba9969d9")
	)
	(pad "3" thru_hole oval
		(at 7.5 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b1f9ec58-aeb1-486d-a43b-b473382cc767")
	)
	(pad "4" thru_hole oval
		(at 10 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "64183966-e8c1-436f-a50e-416c53e59db1")
	)
	(pad "5" thru_hole oval
		(at 12.5 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5ea7d51b-34a6-4ebf-81d7-7342b71b4bdd")
	)
	(pad "6" thru_hole oval
		(at 15 0.5)
		(size 2 3.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "8a7bf802-6b23-497e-987f-40a3869a0307")
	)
	(model "U:/IO-Adapter/custom-kicad-library/3d-models/WAGO_733-366 Print-Stiftleiste Micro RM 2.5 gewinkelt 6-pol.stp"
		(offset
			(xyz 17.6 -0.5 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
