( pcb2gcode 2.5.0 )
( Software-independent Gcode )

( This file uses 1 drill bit sizes. )
( Bit sizes: [2mm] )

G94       (Millimeters per minute feed rate.)
G21       (Units == Millimeters.)
G90       (Absolute coordinates.)
G00 S20000     (RPM spindle speed.)

G00 Z30.00000 (Retract)
T1
M5      (Spindle stop.)
G04 P1.00000
(MSG, Change tool bit to drill size 2mm)
M6      (Tool change.)
M0      (Temporary machine stop.)
M3      (Spindle on clockwise.)
G0 Z2.60000
G04 P1.00000

G81 R2.60000 Z-1.90000 F200.00000 X-92.11720 Y3.83296
X-66.20920 Y37.23396
X-92.11720 Y83.33496
X-58.05620 Y65.22496
X-29.96320 Y68.11996
X-3.97920 Y83.46196
X-21.63220 Y24.02596
X-3.97920 Y3.83296
G80

G00 Z30.000 ( All done -- retract )

M5      (Spindle off.)
G04 P1.000000
M9      (Coolant off.)
M2      (Program end.)

